**Appendix 1 to the Tender Specification EMSA/NEG/18/2016**

|  |  |  |  |
| --- | --- | --- | --- |
| **Types of construction works to be executed within the Framework Contract (Prices per m²) \*** | | **Unit** | **Unit price** |
| a) | Protection of the areas to be refurbished with corrugated cardboard or plastic roll. | m² |  |
| b) | Transportation, assembly and dismantling of scaffolding for works from 3 to 8 meters in height. | m² |  |
| c) | Repair of walls and ceilings in plaster (traditional or projected) including the filling of cracks, correction of deformations and all the work necessary for surface levelling. | m² |  |
| d) | Delivery and application of primer aqueous sealer to interior walls and ceilings with traditional stucco features or plasterboard. | m² |  |
| e) | Delivery and application of aqueous primer sealer to walls and exterior ceilings. | m² |  |
| f) | Application of two coats of water-based paint to interior walls and ceilings with traditional plaster or plasterboard characteristics. | m² |  |
| g) | Supply and application of two coats of acrylic-based paint to exterior walls and ceilings. | m² |  |
| h) | Sanding of wood surfaces, supply and application of two coats of synthetic varnish. | m² |  |
| i) | Sanding of wood surfaces, supply and application of two coats of cellulosic varnish. | m² |  |
| j) | Supply and installation of acoustic insulation, 3.5cm thick, respecting existing lighting sternotomy (STIER-Baswaphon Classic or ROCKFON-Monoacoustic material). | m² |  |
| k) | Removal of dropped- ceilings in micro-perforated plates, including the ceiling support structure. | m² |  |
| l) | Construction of ceilings in plasterboard with metal structure. | m² |  |
| m) | Construction of single partition walls with glass wool insulation 4mm thick, in plasterboard with the metal structure for the partition walls. | m² |  |
| n) | Construction of double-sided partition walls with glass wool insulation 4mm thick, in plasterboard with the metal structure for the partition walls. | m² |  |

\* The price offer must be **all inclusive** (include the costs of transport, all workmanships and materials to be used).

**Appendix 2 to the Tender Specification EMSA/NEG/18/2016**

**For Evaluation purposes**:

|  |  |  |
| --- | --- | --- |
| Proposed **deadlines** (N. of days) for the **start** of the following works **after request**: | M2 | **Deadline** (Days) |
| Delivery and application of primer aqueous sealer to interior walls and ceilings with traditional stucco features or plasterboard. | 100 m² |  |
| Supply and installation of acoustic insulation, 3.5cm thick, respecting existing lighting sternotomy (STIER-Baswaphon Classic or ROCKFON-Monoacoustic material). | 250 m² |  |
| Construction of double-sided partition walls with glass wool insulation 4mm thick, in plasterboard with the metal structure for the partition walls. | 30 m² |  |