|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for Standard Office Chair** | | **Compliance**  **YES/NO** | **Comments:** |
| 1. **Certifications & declarations** | | | |
| 1.a | Declaration of conformity according to: EN 1335-1(2000), 2 and 3 (2009), EN ISO 9241-5 (1999) |  |  |
| 1.b | Quality certificate to: EN 1335-1(2000), 2 and 3 (2009), EN ISO 9241-5 (1999) and  XPD 61040-4 (1997) |  |  |
| 1.c | Test according with BS 5459-2:2000+A2:2008 |  |  |
| 1.d | Material certifications regarding (i.e. eco-labels) |  |  |
| 1.e | Environment product declaration |  |  |
| 1. **Mandatory features of standard office chair** | | | |
| 2.a | Colour (blue similar to the colour of the existing furniture) or other surface material on request. |  |  |
| 2.b | Rotating armrests, adjustable 360° |  |  |
| 2.c | Wheels suitable for hard textile surface |  |  |
| 2.d | Aluminium frame |  |  |
| 1. **Price per unit** | | | |
| 3.a | Price per unit |  | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for Ergonomic Chair** | | **Compliance**  **YES/NO** | **Comments:** |
| 1. **Certifications & declarations** | | | |
| 1.a | Declaration of conformity according to: EN 1335-1(2000), 2 and 3 (2009), EN ISO 9241-5 (1999) |  |  |
| 1.b | Quality certificate to: (EN 1335-1(2000), 2 and 3 (2009), EN ISO 9241-5 (1999), XPD 61040-4 (1997) |  |  |
| 1.c | Test according with BS 5459-2:2000+A2:2008 |  |  |
| 1.d | Ergonomics approved certificate/Award |  |  |
| 1.e | Material certifications regarding (i.e. eco-labels) |  |  |
| 1.f | Environment product declaration |  |  |
| 1.g | Contribution to LEED |  |  |
| 1. **Mandatory features of ergonomic chair** | | | |
| 2.a | Aluminium frame |  |  |
| 2.b | Colour (blue similar to the colour of the existing furniture) or other surface material on request. |  |  |
| 2.c | Supplied with head rest |  |  |
| 2.d | Wheels suitable for hard textile surface |  |  |
| 1. **Price per unit** | | | |
| 3.a | Price per unit |  | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for Standard Visitor Chair** | | **Compliance**  **YES/NO** | **Comments:** |
| 1. **Certifications & declarations** | | | |
| 1.a | Declaration of conformity according to:  EN16139 (2013) level 1 compatible |  |  |
| 1.b | Quality certificate to:  EN 1335-1(2000), 2 and 3 (2009) and EN ISO 9241-5 |  |  |
| 1.c | Environment product declaration |  |  |
| 1.d | Contribution to LEED |  |  |
| 1. **Mandatory features of visitor chair** | | | |
| 2.a | Stackable |  |  |
| 2.b | Colour (blue similar to the colour of the existing furniture) or other surface material on request. |  |  |
| 2.c | Proposed model with arm rest |  |  |
| 2.d | Proposed model without arm rest |  |  |
| 1. **Price per unit** | | | |
| 3.a | Price per unit |  | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for Electric Adjustable Office Table** | | **Compliance**  **YES/NO** | **Comments:** |
| 1. **Certifications & declarations** | | | |
| 1.a | Declaration of conformity according to: EN 527-1 (2011), EN 527-2 (2002), EN 527-3 (2003), EN 60335-1 (2010), 2006/42 EC, 2006/95 EC and 2004/108/EC from December |  |  |
| 1.b | Quality certificate to: EN 527-1 (2011), EN 527-2 (2002), EN 527-3 (2003), XP D62042 (2010) and EN ISO 9241-5 (1999) |  |  |
| 1.c | Material certifications |  |  |
| 1.d | Environment product declaration |  |  |
| 1.e | Cradle to cradle certified |  |  |
| 1. **Mandatory features of electric adjustable office table (5% deviation will be accepted)** | | | |
| 2.a | Melamine surface construction 25mm thick |  |  |
| 2.b | Wood colour of desk top: "Bahia" (Proposed colour of the wood should be similar to the colour of the table top in the attached picture - Appendix 3) |  |  |
| 2.c | Antibacterial treated surface |  |  |
| 2.d | Two access openings for cabling passage |  |  |
| 2.e | Cabling support structure under the top- colour dark grey |  |  |
| 2.f | High-density wood chipboard, covered with natural mahogany leaf, finishing in matt varnish |  |  |
| 1. **Structure of frame** | | | |
| 3.a | Metal base |  |  |
| 3.b | Colour: Silver |  |  |
| 3.c | Adjustable frame features |  |  |
| 3.d | Electric power to lift and adjust the work surface height by users |  |  |
| 3.e | Power cable minimum 3 meters |  |  |
| 1. **Dimensions and weight ( 5% deviation will be accepted)** | | | |
| 4.a | Dimensions: 1800mm (width) x 800mm (depth) |  |  |
| 4.b | Adjustable working height from 650mm to 1250mm |  |  |
| 4.c | Weight able to support: 75 kg (approximately) |  |  |
| 4.d | Compatible PC holder |  |  |
| 4.e | Metal PC Holder compatible with the electric table |  |  |
| 4.f | Weight able to support: 15 kg (approximately) |  |  |
| 4.g | Colour: dark grey |  |  |
| 1. **Price per unit** | | | |
| 5.a | Price per unit |  | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for Seated table** | | **Compliance**  **YES/NO** | **Comments:** |
| 1. **Certifications & declarations** | | | |
| 1.a | Declaration of conformity according to: EN 527-1 (2011) |  |  |
| 1.b | Quality certificate |  |  |
| 1.c | Environment product declaration |  |  |
| 1. **Mandatory features of seated table** | | | |
| 2.a | Melamine surface construction 30mm thick |  |  |
| 2.b | Wood colour of desk top: "Bahia" (Proposed colour of the wood should be similar to the colour of the table top in the attached picture - Appendix 3) |  |  |
| 2.c | High-density wood chipboard, covered with natural mahogany leaf, finishing in matt varnish |  |  |
| 2.d | Two access openings for cabling passage |  |  |
| 2.e | Cabling support structure under the top |  |  |
| 1. **Structure of frame** | | | |
| 3.a | Metal base |  |  |
| 3.b | Colour: Silver |  |  |
| 3.c | Adjustable frame features |  |  |
| 1. **Dimensions and weight ( 5% deviation will be accepted)** | | | |
| 4.a | Dimensions: 1800mm (width) x 800mm (depth) |  |  |
| 4.b | Adjustable working height from 650mm to 1250mm |  |  |
| 4.c | Weight able to support: 75 kg (approximately) |  |  |
| 1. **Price per unit** | | | |
| 5.a | Price per unit |  | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for Cupboards** | | **Compliance**  **YES/NO** | **Comments:** |
| 1. **Certifications & declarations** | | | |
| 1.a | Independent verification of the environmental declaration (EPD - ISO/TR 14025) |  |  |
| 1.b | Contribution to LEED |  |  |
| 1.c | Environment product declaration |  |  |
| 1. **Mandatory features of Cupboards** | | | |
| 2.a | Side opening tambour doors, colour grey, similar to the existing model |  |  |
| 2.b | Interior equipment: 4/5 shelves |  |  |
| 2.c | Lock and minimum 2 keys |  |  |
| 1. **Dimensions (5% deviation will be accepted)** | | | |
| 3.a | Height: 2000mm |  |  |
| 3.b | Width: 1000mm |  |  |
| 3.c | Depth: 430mm |  |  |
| 1. **Price per unit** | | | |
| 4.a | Price per unit |  | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for Low Cupboards** | | **Compliance**  **YES/NO** | **Comments:** |
| 1. **Certifications & declarations** | | | |
| 1.a | Independent verification of the environmental declaration (EPD - ISO/TR 14025) |  |  |
| 1.b | Contribution to LEED |  |  |
| 1.c | Environment product declaration |  |  |
| 1. **Mandatory features of Low Cupboards** | | | |
| 2.a | Side opening tambour doors, colour grey, wood top colour: "Bahia" (Proposed colour of the wood should be similar to the attached picture - Appendix 3) similar to the existing model |  |  |
| 2.b | Interior equipment: 1 shelf |  |  |
| 2.c | Lock and minimum 2 keys |  |  |
| 1. **Dimensions (5% deviation will be accepted)** | | | |
| 3.a | Height: 870mm |  |  |
| 3.b | Width: 1000mm |  |  |
| 3.c | Depth: 450mm |  |  |
| 1. **Price per unit** | | | |
| 4.a | Price per unit |  | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for Rolling Cupboards** | | **Compliance**  **YES/NO** | **Comments:** |
| 1. **Certifications & declarations** | | | |
| 1.a | Quality certificate to: EN 14073 1/2/3 (2005), EN 14074 (2005), NF D 62-041 (2011), NF D 60050 (2009) |  |  |
| 1.b | Environment product declaration |  |  |
| 1.c | Contribution to LEED |  |  |
| 1. **Mandatory features of Rolling Cupboards** | | | |
| 2.a | with 3 drawers |  |  |
| 2.b | Lock and 2 keys |  |  |
| 1. **Dimensions (5% deviation will be accepted)** | | | |
| 3.a | Height: 550mm |  |  |
| 3.b | Width: 415mm |  |  |
| 3.c | Depth: 595mm |  |  |
| 1. **Price per unit** | | | |
| 4.a | Price per unit |  | |

|  |  |  |
| --- | --- | --- |
| 1. **Price per man hour for maintenance** | | |
| 1.a | Price per man hour for maintenance services |  |